124th W Notes
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Notes from field. Monument not used. 
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Notes from field. 
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Picture showing the placement of the guard rail bolt used as SVPA local benchmark. 
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Up close image of bolt used as SVPA local benchmark. 
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Info from archives:

Flood Sensor Location #15 - NE 124th St Bridge at Snogualmie River

T

KING COUNTY SURVEY INFO

Date of Survey: 09-05-18

BULIH Ul FOUSIN EreVaLioi: 93,04

Bridge Deck Elevation: 60.86

E = 1354463.69, Elevation: 60.33

37 Brass Monument: N = 260799.30,

Set Mag Nail: N = 260759.44, € = 1354786.31, Elevation: 55.04

Comments: Basis of bearing 589°24'32"E, 1379.98'

T 0F Stadon Yo s b \D
Top of Sorse 1o boftom 33

paher o sersor IEGEEN





image2.png
129 W

Field Worksheet >
Point Description Level Upper Lower  (offset)  Height  Elevation Range
Two peg test
Setup A Instrament equidestint between pegs
Peg 1
Peg 2
True difference in elevation
Setup B Instrament near Point 1
Peg 1
Peg 2
Aparent difference in elevation
Elevation Error
Error per 100 feet
1 (Known Elevation) ,I
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