Sno Falls Golf
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Data from 12/31/2020 Survey at SFG including calibration. 
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Notes from field. 
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Images of the SVPA Local Bench Mark used at Sno Falls Golf. The top of the bolt, as shown above and in the circle to the left, on the post directly in front of the sensor post is the BM. 
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Field Worksheet
Point Description Upper  Lower  |(offsety  Height  Elevation Range

Two peg test

Instrament equidestint between pegs

Setup A
peg1 Nerfl

4 350 4.555

Pegz S k4,450, ¢, 560| ¢, 515
True diference in elevation

Setup B Instrament near Point 1

v

Peg2 S

Peg 1 |.845 U568
Aparent dierence in elevation

Elevation Error

Error per 100 feet

(Known Elevation)
7 Iy

Setwp1 A V0@

SVPA Location Benchmark

PM1
PM2
Sensor

Ground dry ground under sensor

Road Saddle
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