Tolt Bridge Survey 12/31/2020
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Illustrating survey points, starting with the King County monument described on sticky note; and ending with the SVPA local benchmark which is the concrete ledge of the bridge as shown in pictures below. 
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My documentation of location of sensor, determined while out on bridge. 
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Picture showing location of sensor. Sensor is hanging off bridge behind the leveling rod. 
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Part of bridge used as SVPA Local BM.
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Notes from survey. 
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Field Worksheet

Elevation | Range

Description Level Upper  Lower (offset)  Height

Instrament equidestint between pegs

True difference in elevation

Instrament near Point 1

Aparent difference in elevation
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